LIVEMIX MIX-16/32 VERSION HISTORY 

v4.0
Update to Dante Firmware v4 to enable support for Dante Domain Manager
Remove the ability to subscribe to Dante channels with the CS-DUO or CS-SOLO. Channel assignment and subscription is made with the free Dante Controller from Audinate.
Product compatibility updates

2.19
Product compatibility updates
 
2.18
Product compatibility updates


V2.15
Added support for LM-MICPRE for using external dynamic microphone with intercom.
   Added LM-MICPRE functionality to Intercom Channel Single Channel View
   Added LM-MICPRE configuration screen to Intercom Channel Single Channel View
Added ability to group Accessory Channels
Added Global MirrorMix feature
Added passcode support for Global MirrorMix feature
Various bug fixes and improvements

v2.1
Add support for Dante Device Lock and AES67 (Some functionality related to Dante Device Lock and AES67 requires use of Dante Controller).
Support Dante "Identify Device" function by flashing MIX-16/32 Livemix Data LED and LM-DANTE-EXP RJ-45 LEDs.
    
v2.02
Various bug fixes and improvements

v2.0
Updated DA-816 identification handshake and identification process.
Added support for CS-SOLO
Release of MirrorMix 2.0 featuring:
  MirrorMix port selection screen allows remote mix audition upon port selection.
  New MirrorMix Functions menu adds quick setup and "push" options: Push Current Mix, Push Master Output Settings, Push Groups, Push Saved Mix
  Intercom directly to remote mixer in MirrorMix mode
  Selected MirrorMix port displayed on top of LCD screen
Remove the ability for MIX-16/32 to report as audio input device to PCs 
Various bug fixes and improvements

v1.16
Added support for DA-816
Improved diagnostic instructions added to "MIX-16 Communication Error" pop-up
Make MIX-32 LEDs more closely match MIX-16 LEDs during power-up
Fix Windows 8 / Windows 10 issues in MIX-16 update wizard

v1.12
Default to Dante mode on first power-up if Dante module is installed
Increase number of supported Dante devices from 16 to 32
Deactivate “Mute” and “Solo” when loading a mix
Deactivate ganging of A and B sides when loading a mix or at power-up
Allow MIX-16/32 update from CS-DUO
Rescale CS-DUO VU indicators so green indicator turns on at -40dBFS instead of -20dBFS
Add support for MIX-32
Various bug fixes and improvements



SUPPORT
http://digitalaudio.com/support/